Riveting the first planks

Insert a cable tie through the hole in the plank on the top and through the matching hole in the bottom plank.

From the outside of the hull, slide another cable tie over the tail of the first one, completing the rivet. Leave the rivets loose at this point. Pivot the two planks together until the next pair of holes line up, and repeat the riveting process.
[ Back - Menu - Next ]