Final riveting checks

When you are finished admiring what you have accomplished so far, assemble the other half using the same method. Remember that the second half is a mirror of the first, and that when you put the two halves of the hull together that you want the scarfs at the same ends of each pair of panels.

After the second half is completely assembled, check to make sure that all the laps are on the correct side, that all the gains are on the outside, and that everything lines up correctly. When everything checks out OK, begin to stitch the two halves together along the keel line.
[ Back - Menu - Next ]